
# Auto generated by RootStock-NG: setup_sdcard.sh
# udevadm info -q all -p /sys/class/net/eth0 --attribute-walk

# BeagleBone: net device ()
SUBSYSTEM=="net", ACTION=="add", DRIVERS=="?*", ATTR{dev_id}=="0x0", ATTR{type}=="1", KERNEL=="eth*", NAME="eth0"

# BeagleBone: net device ()
SUBSYSTEM==net, ACTION==add, DRIVERS==?*, ATTR{dev_id}==0x0, ATTR{type}==1, KERNEL==eth*, NAME=eth0

# USB device 0x:0x (ath9k_htc)
#SUBSYSTEM=="net", ACTION=="add", DRIVERS=="?*", ATTR{address}=="c4:6e:1f:10:de:b1", ATTR{dev_id}=="0x0", ATTR{type}=="1", KERNEL=="wlan*", NAME="wlan0"

# USB device 0x:0x (rt73usb)
#SUBSYSTEM=="net", ACTION=="add", DRIVERS=="?*", ATTR{address}=="94:44:52:03:5e:76", ATTR{dev_id}=="0x0", ATTR{type}=="1", KERNEL=="wlan*", NAME="wlan1"
