# do not edit this file, it will be overwritten on update

ACTION!="add|change|move", GOTO="mm_telit_port_types_end"
SUBSYSTEM!="tty", GOTO="mm_telit_port_types_end"

SUBSYSTEMS=="usb", ATTRS{idVendor}=="1bc7", GOTO="mm_telit_vendorcheck"
GOTO="mm_telit_port_types_end"

LABEL="mm_telit_vendorcheck"
SUBSYSTEMS=="usb", ATTRS{bInterfaceNumber}=="?*", ENV{.MM_USBIFNUM}="$attr{bInterfaceNumber}"

# UC864-E, UC864-E-AUTO, UC864-K, UC864-WD, UC864-WDU
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1003", ENV{.MM_USBIFNUM}=="00", ENV{ID_MM_TELIT_PORT_TYPE_MODEM}="1"
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1003", ENV{.MM_USBIFNUM}=="02", ENV{ID_MM_TELIT_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1003", ENV{ID_MM_TELIT_TAGGED}="1"

# UC864-G
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1004", ENV{.MM_USBIFNUM}=="00", ENV{ID_MM_TELIT_PORT_TYPE_MODEM}="1"
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1004", ENV{.MM_USBIFNUM}=="02", ENV{ID_MM_TELIT_PORT_TYPE_NMEA}="1"
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1004", ENV{.MM_USBIFNUM}=="03", ENV{ID_MM_TELIT_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1004", ENV{ID_MM_TELIT_TAGGED}="1"

# CC864-DUAL
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1005", ENV{.MM_USBIFNUM}=="00", ENV{ID_MM_TELIT_PORT_TYPE_MODEM}="1"
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1005", ENV{.MM_USBIFNUM}=="02", ENV{ID_MM_TELIT_PORT_TYPE_NMEA}="1"
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1005", ENV{.MM_USBIFNUM}=="03", ENV{ID_MM_TELIT_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1005", ENV{ID_MM_TELIT_TAGGED}="1"

# CC864-SINGLE, CC864-KPS
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1006", ENV{.MM_USBIFNUM}=="00", ENV{ID_MM_TELIT_PORT_TYPE_MODEM}="1"
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1006", ENV{.MM_USBIFNUM}=="02", ENV{ID_MM_TELIT_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1006", ENV{ID_MM_TELIT_TAGGED}="1"

# DE910-DUAL
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1010", ENV{.MM_USBIFNUM}=="01", ENV{ID_MM_TELIT_PORT_TYPE_NMEA}="1"
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1010", ENV{.MM_USBIFNUM}=="02", ENV{ID_MM_TELIT_PORT_TYPE_AUX}="1"
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1010", ENV{.MM_USBIFNUM}=="03", ENV{ID_MM_TELIT_PORT_TYPE_MODEM}="1"
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1010", ENV{ID_MM_TELIT_TAGGED}="1"

# CE910-DUAL
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1011", ENV{.MM_USBIFNUM}=="01", ENV{ID_MM_TELIT_PORT_TYPE_MODEM}="1"
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1011", ENV{ID_MM_TELIT_TAGGED}="1"

# HE910, UE910, UL865 (dynamic port identification supported)
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="0021", ENV{ID_MM_TELIT_TAGGED}="1", ENV{ID_MM_TELIT_PORTS_TAGGED}="1"

# LE910 V2
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="0036", ENV{ID_MM_TELIT_TAGGED}="1", ENV{ID_MM_TELIT_PORTS_TAGGED}="1"

# LE910 V2
ATTRS{idVendor}=="1bc7", ATTRS{idProduct}=="1201", ENV{ID_MM_TELIT_TAGGED}="1", ENV{ID_MM_TELIT_PORTS_TAGGED}="1"

# NOTE: Qualcomm Gobi-based devices like the LE920 should not be handled
# by this plugin, but by the Gobi plugin.

GOTO="mm_telit_port_types_end"
LABEL="mm_telit_port_types_end"
